;; This buffer is for text that is not saved, and for Lisp evaluation.
;; To create a file, visit it with C-x C-f and enter text in its buffer.


FIR1
total sim-cycles = 6,011
total frames = 6,010
total stages = 597
total instructions = 199
max energy = 1430
avg energy = 758
max stage period = 18
avg stage period = 10
port 0 , samples = 13 , sim-cycles = 5,664 , sample-period = 435.000
port 1 , samples = 13 , sim-cycles = 5,979 , sample-period = 459.000

FIR2
total sim-cycles = 5,639
total frames = 5,638
total stages = 597
total instructions = 199
max energy = 1430
avg energy = 796
max stage period = 18
avg stage period = 9
port 0 , samples = 24 , sim-cycles = 5,439 , sample-period = 226.000
port 1 , samples = 24 , sim-cycles = 5,523 , sample-period = 230.000


